For 1990-2009 cars

The entertainment system consists of a radio, 4 speakers, and an antenna.

The following lists the available entertainment system options:

• | An AM/FM stereo radio with a clock

• | An AM/FM stereo radio with an auto-reverse tape player and a clock

• | An AM/FM stereo with a compact disc player and a clock

The ignition switch must be in the ACC or ON position in order to operate any of the sound systems. The front speakers are located on the front doors. The rear speakers are located beneath the rear quarter lower trim panel on each side of the vehicle.

### FM Radio Reception

The FM tuner operates on a band from 87.7-107.9 MHz. Optimum FM radio reception range is usually limited to a maximum of 16-64 km (10-40 miles) depending on terrain, atmospheric conditions, station power, antenna height and distance from the transmitter. Tall buildings, hills or other objects can case signal flutter or noise. Eliminate the noise by tuning to a stronger station.

### AM Radio Reception

The AM tuner operates on a band from 530-1710 kHz. The range of most AM stations is greater than FM, especially at night. AM signals can interfere with each other due to the longer range of the AM band. AM reception is subject to noise interference from storms and power lines. Reduce the treble in order to reduce noise.