For 1990-2009 cars

## Fastener Tightening Specifications 4WD

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Clutch Housing Bolts | 45 N·m | 33 lb ft
Countershaft Center Bearing Plate Bolts | 10 N·m | 89 lb in
Gearshaft Lever Case Bolts | 17 N·m | 13 lb ft
Input Shaft Bearing Retainer Bolts | 23 N·m | 17 lb ft
Lever Locating Bolts | 20 N·m | 15 lb ft
Locating Spring Bolts | 28 N·m | 21 lb ft
Rear Case Bolts | 23 N·m | 17 lb ft
Reverse Gearshift Limit Bolt | 35 N·m | 26 lb ft
Reverse Idler Shaft Bolt | 22 N·m | 16 lb ft
Select Return Spring Bolts | 23 N·m | 17 lb ft
Transfer Case-to-Transmission Bolts | 28 N·m | 21 lb ft
Upper-to-Lower Case Retaining Bolts | 23 N·m | 17 lb ft

## Fastener Tightening Specifications 2WD

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 20 N·m | 15 lb ft
Clutch Housing Bolts | 45 N·m | 33 lb ft
Countershaft Center Bearing Plate Bolts | 6 N·m | 53 lb in
Extension Case Bolts | 23 N·m | 17 lb ft
Gearshift Lever Case Bolts | 17 N·m | 13 lb ft
Input Shaft Bearing Retainer Bolts | 23 N·m | 17 lb ft
Lever Locating Bolts | 20 N·m | 15 lb ft
Locating Spring Bolts | 28 N·m | 21 lb ft
Reverse Gearshift Limit Bolt | 35 N·m | 26 lb ft
Reverse Idler Shaft Bolt | 22 N·m | 16 lb ft
Select Return Spring Bolts | 23 N·m | 17 lb ft
Speedometer Driven Gear Case Retaining Bolt | 12 N·m | 106 lb in
Upper-to-Lower Case Retaining Bolts | 23 N·m | 17 lb ft

Application | Specification
--- | ---
Metric | English
Backup Lamp Switch | 23 N·m | 17 lb ft
Clutch Release Lever Bolt and Nut | 24 N·m | 17 lb ft
Extension Case Bolts | 28 N·m | 20 lb ft
Fan Shroud Bolt | 10 N·m | 89 lb in
Flywheel Inspection Cover Bolt | 10 N·m | 89 lb in
Front Skid Plate Bolt | 54 N·m | 40 lb ft
Gearshift Control Lever Lower Boot Plate Bolt | 7 N·m | 62 lb in
Gearshift Lever Case Bolt | 17 N·m | 12 lb ft
Left Transmission-to-Engine Reinforcement Brace Bolt | 100 N·m | 72 lb ft
Lever Locating Bolt | 20 N·m | 15 lb ft
Lower Transmission-to-Engine Nut | 100 N·m | 72 lb ft
Rear Case Bolt (Four-Wheel Drive Models) | 28 N·m | 20 lb ft
Rear Propeller Shaft Bolt and Nut (Two-Wheel Drive Models) | 50 N·m | 37 lb ft
Rear Transmission Crossmember Bolt (Two-Wheel Drive Models) | 60 N·m | 44 lb ft
Rear Transmission Mount Bolt (Two-Wheel Drive Models) | 60 N·m | 44 lb ft
Reverse Gearshift Limit Bolt | 35 N·m | 26 lb ft
Right Transmission-to-Engine Reinforcement Brace Bolt | 100 N·m | 72 lb ft
Select Return Spring Bolt | 32 N·m | 24 lb ft
Speedometer Driven Gear Case Bolt | 12 N·m | 106 lb in
Starter Motor Bolts and Nut | 30 N·m | 22 lb ft
Transmission Drain Plug | 28 N·m | 20 lb ft
Transmission Oil Lever/Filler Plug | 28 N·m | 20 lb ft
Upper Transmission-to-Engine Bolt | 100 N·m | 72 lb ft