For 1990-2009 cars

The rear side door lock assembly on the four-door models incorporates a rear door child security lock. The child security locks (3) are engaged and disengaged with a switch built into the lock assembly (2). With the switch engaged, only the outside handle opens the rear side door. Service the rear door child security locks (3) as a part of the lock assembly (2), not separately.