For 1990-2009 cars

### Removal Procedure

1. Remove the IP cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement in Instrument Panel, Gages and Console.
2. Using a taped flat bladed tool, gently pry the rear window defogger switch (1) from the instrument panel.
3. Disconnect the rear window defogger switch electrical connector (2).
4. Remove the switch (1) from the vehicle.

### Installation Procedure

1. Connect the rear window defogger switch electrical connector (2).
2. Install the rear window defogger switch (1) to the instrument panel. Ensure that the retaining tabs are fully engaged.
3. Install the IP cluster trim plate. Refer to Instrument Panel Cluster Trim Plate Bezel Replacement in Instrument Panel, Gages and Console.