For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
2. Release the retaining tab on the bottom of the rear wiper/washer switch by pushing it up with a pick.
3. Slide out the rear wiper/washer switch from the instrument panel.
4. Disconnect the electrical connector from the rear wiper/washer switch.
5. Remove the rear wiper/washer switch from the vehicle.

### Installation Procedure

1. Connect the electrical connector to the rear wiper/washer switch.
2. Install the rear wiper/washer switch to the instrument panel. Ensure that the retaining tabs are fully engaged.
3. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.