For 1990-2009 cars

### Removal Procedure

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

2. Disconnect the negative battery cable.

Caution: To avoid any vehicle damage, serious personal injury or death when major components are removed from the vehicle and the vehicle is supported by a hoist, support the vehicle with jack stands at the opposite end from which the components are being removed and strap the vehicle to the hoist.

3. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
4. Disconnect the fuel inlet hose (2) from the fuel filter (1).
5. Disconnect the fuel outlet hose (4) from the fuel filter (1).
6. Remove the retaining bolt (3) from the fuel filter bracket .
7. Remove the fuel filter (1) and the bracket from the vehicle.
8. Loosen the fuel filter bracket bolt and remove the fuel filter from the bracket.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the fuel filter to the fuel filter bracket.

Tighten
Tighten the bracket bolt to 11 N·m (8 lb ft).

2. Install the fuel filter (1) and the bracket to the vehicle.
3. Secure the fuel filter bracket to the vehicle with the retaining bolt (3).

Tighten
Tighten the bracket retaining bolt to 11 N·m (8 lb ft).

4. Reconnect the fuel outlet hose (4) to the fuel filter (1).
5. Reconnect the fuel inlet hose (2) to the fuel filter.
6. Lower the vehicle.
7. Connect the negative battery cable.
8. Start the engine.
9. Inspect for fuel leaks and repair as necessary.