For 1990-2009 cars

### Removal Procedure

1. Remove the front side door window. Refer to Front Side Door Window Replacement .
2. Disconnect the front side door window regulator electrical connector, if equipped.
3. Remove the 4 bolts (1) and the 3 nuts (2) which secure the front side door window regulator.
4. Remove the window regulator through the large opening in the inner portion of the front side door (3).

### Installation Procedure

1. Apply a multipurpose grease to the specified points.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the front side door window regulator through the large opening in the inner portion of the front side door (3). Secure the regulator to the door with the 4 bolts (1) and the 3 nuts (2).

Tighten
Tighten the front side door window regulator bolts and nuts to 10 N·m (89 lb in).

3. Connect the front side door window regulator electrical connector, if equipped.
4. Install the front side door window. Refer to Front Side Door Window Replacement .