For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner (ACL) Mounting Bolts | 10 N·m | 89 lb in
Air Conditioner (A/C) Compressor Flexible Hose Mounting Bolts | 10 N·m | 89 lb in
Air Conditioner (A/C) Mounting Bracket Bolts | 10 N·m | 89 lb in
Air Intake Pipe Bolts | 10 N·m | 89 lb in
Air Intake Pipe Bracket Bolts | 15 N·m | 11 lb ft
Camshaft Housing Bolts | 10 N·m | 89 lb in
Camshaft Sensor Bolt | 10 N·m | 89 lb in
Camshaft Sensor Housing Bolts | 10 N·m | 89 lb in
Camshaft Timing Sprocket Bolt | 60 N·m | 44 lb ft
Connecting Rod Bearing Cap Nuts | 35 N·m | 26 lb ft
Coolant Intake Pipe Bolt | 11 N·m | 97 lb in
Coolant Pump Bolts | 12 N·m | 106 lb in
Coolant Pump Pulley Nuts | 11 N·m | 97 lb in
Crankshaft Pulley Bolts | 16 N·m | 12 lb ft
Crankshaft Timing Sprocket Bolt | 110 N·m | 81 lb ft
Cylinder Head Bolts

- First Pass

35 N·m

26 lb ft

- Second Pass

55 N·m

41 lb ft

- Third Pass (Final Torque)

70 N·m

52 lb ft

Cylinder Head Cover Bolts | 10 N·m | 89 lb in
Engine Mount Bracket Bolts (Engine Side) | 50 N·m | 37 lb ft
Engine Mount Bracket Bolts (Body Side) | 85 N·m | 62 lb ft
Engine Mount Nuts | 50 N·m | 37 lb ft
Engine Oil Drain Plug | 35 N·m | 26 lb ft
Engine Oil Pan Nuts and Bolts | 11 N·m | 97 lb in
Exhaust Bracket-to-Exhaust Manifold Nut | 50 N·m | 37 lb ft
Exhaust Manifold Nuts | 23 N·m | 17 lb ft
Exhaust Manifold Heat Shield Bolts and Nuts | 10 N·m | 89 lb in
Exhaust Manifold-to-Cylinder Head Bolts and Nuts | 23 N·m | 17 lb ft
Exhaust Manifold-to-Front Pipe/Three Way Catalytic Converter (TWC) Assembly Bolts | 50 N·m | 37 lb ft
Exhaust Pipe-to-Bracket Nut | 50 N·m | 37 lb ft
Fan Clutch Nuts | 11 N·m | 97 lb in
Flywheel Retaining Bolts | 78 N·m | 58 lb ft
Front End Panel Bolts | 10 N·m | 89 lb in
Front Pipe/TWC Assembly-to-Exhaust Manifold Bolts | 50 N·m | 37 lb ft
Front Pipe/TWC Assembly-to-Resonator/Center Pipe Nuts | 35 N·m | 26 lb ft
Front Skid Plate Bolts | 55 N·m | 40 lb ft
Generator Adjusting Arm Bracket Nut and Bolt | 23 N·m | 17 lb ft
Generator Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Guide Tube Bolts | 14 N·m | 10 lb ft
Heated Oxygen (HO2S1) Sensor | 43 N·m | 32 lb ft
Hood Latch Bolts | 10 N·m | 89 lb in
Ignition Coil Bolts | 3 N·m | 27 lb in
Intake Manifold Nuts and Bolts | 23 N·m | 17 lb ft
Intake Manifold Support Bracket Bolts | 50 N·m | 37 lb ft
Main Bearing Cap Bolts | 54 N·m | 40 lb ft
Oil Jet | 5 N·m | 44 lb in
Oil Pressure Switch | 14 N·m | 10 lb ft
Oil Pump Bolts | 11 N·m | 97 lb in
Oil Pump Strainer Bolt | 11 N·m | 97 lb in
Oil Pump Strainer Bracket Bolt | 11 N·m | 97 lb in
Rear Main Seal Housing Bolts | 12 N·m | 106 lb in
Rocker Arm Shaft Bolts | 10 N·m | 89 lb in
Rocker Arm Shaft Plug | 33 N·m | 24 lb ft
Shroud Bolts | 11 N·m | 97 lb in
Timing Belt Cover Nut and Bolts | 10 N·m | 89 lb in
Timing Belt Inside Cover Bolts | 10 N·m | 89 lb in
Timing Belt Tensioner Bolt | 27 N·m | 20 lb ft
Timing Belt Tensioner Stud | 11 N·m | 97 lb in
Throttle Body Nuts and Bolts | 23 N·m | 17 lb ft
Throttle Cover Bolts | 15 N·m | 11 lb ft