For 1990-2009 cars

### Removal Procedure

1. Push both sides of the glove box in towards the center (3).
2. Pull the glove box down.
3. Disconnect the main relay electrical connector.
4. Remove the main relay (2) from the bracket.

### Installation Procedure

1. Install the main relay (2) to the bracket.
2. Connect the main relay electrical connector.
3. Push the glove box up and back into the closed position.