For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Blower Case Retaining Bolts | 10 N·m | 89 lb in
Clutch Coil Wire Retainer Bolt | 2-2.5 N·m | 17.7-22.12 lb in
Compressor Discharge Hose Bolt | 25 N·m | 19 lb ft
Compressor Lower Bracket-to-Engine Bolts (1.6L) | 18-25 N·m | 13-20 lb ft
Compressor Mounting Bolts | 23 N·m | 17 lb ft
Compressor Mounting Bracket Bolts (2.0L) | 23 N·m | 17 lb ft
Compressor Suction Hose Bolt | 25 N·m | 19 lb ft
Compressor Upper Bracket-to-Engine Bolts (1.6L) | 40-60 N·m | 29-43 lb ft
Condenser Inlet Pipe Fitting Bolt | 25 N·m | 19 lb ft
Condenser Outlet Pipe Fitting Bolt | 35 N·m | 26 lb ft
Condenser Mounting Bolts | 20 N·m | 15 lb ft
Condenser Outlet-to-Evaporator Inlet Pipe Nut | 25 N·m | 19 lb ft
Evaporator Case Mounting Bolts and Nut | 10 N·m | 89 lb in
Evaporator Outlet-to-Suction Hose Pipe Nut | 35 N·m | 26 lb ft
Expansion Valve Bolt | 35 N·m | 26 lb ft
Heater Case Bolts and Nuts | 10 N·m | 89 lb in
Pressure Plate Nut | 15 N·m | 11 lb ft
Pressure Relief Valve | 12-18 N·m | 8.7-13 lb ft
Receiver/Dryer Cap | 13 N·m | 10 lb ft
Refrigerant Pressure Switch | 18 N·m | 13 lb ft