For 1990-2009 cars

### Removal Procedure

1. Gently pry the inner mirror trim (2) from the door (1).
2. Disconnect the power mirror electrical connector, if equipped.
3. Remove the 3 screws and mirror (4) from the door (1).
4. Remove the outer mirror trim (3) from mirror (4).
5. Remove the gasket from the mirror (4).

### Installation Procedure

1. Install the gasket to the mirror (4).
2. Install the outer mirror trim (3) to the mirror (4).
3. Install the mirror (4) to the door (1). Secure the mirror (4) with the 3 screws.
4. Connect the power mirror electrical connector, if equipped.
5. Install the inner mirror trim (2) to the door (1) by snapping the mirror trim into place.