For 1990-2009 cars

### Removal Procedure

1. Remove the condenser fan relay (3) from the mounting bracket.
2. Remove the rubber sleeve from the condenser fan relay.
3. Disconnect the condenser fan relay from the electrical connector.

### Installation Procedure

1. Connect the condenser fan relay (3) to the electrical connector.

Important: If the rubber sleeve is not correctly installed water and other contaminant intrusion may result and affect proper A/C operation.

2. Install the rubber sleeve to the condenser fan relay.
3. Install the condenser fan relay to the mounting bracket.