For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement .
2. Release the clip-on sides of the power mirror switch by pushing the sides with a pick.
3. Slide out the power mirror switch from the instrument panel.
4. Disconnect the electrical connector from the power mirror switch.

### Installation Procedure

1. Connect the electrical connector to the power mirror switch.
2. Slide the power mirror switch into place.
3. Install the knee bolster. Refer to Knee Bolster Replacement .