For 1990-2009 cars

### Removal Procedure

1. Gently pry the outside rearview mirror opening cover (2) from the front side door.
2. Disconnect the outside rearview mirror electrical connector (1).
3. Remove the 3 bolts (2) and outside rearview mirror (3) from the door.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the outside rearview mirror (3) to the front side door. Secure the mirror with the 3 bolts.

Tighten
Tighten the outside rearview mirror bolts to 10 N·m (89 lb in).

2. Connect the outside rearview mirror electrical connector (1).
3. Install the outside rearview mirror opening cover (2) to the door. Ensure that the plastic retainers are fully engaged.