For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Generator Mounting Bolt | 23 N·m | 17 lb ft
Inner Tie Rod | 85 N·m | 61.5 lb ft
Outer Tie Rod Nut | 43 N·m | 31.5 lb ft
Power Steering Fluid Reservoir Bracket Bolt | 11 N·m | 96 lb in
Power Steering Gear Bracket Bolts | 55 N·m | 40 lb ft
Power Steering Gear Inlet Hose Bolt | 35 N·m | 25.5 lb ft
Power Steering Gear Inlet Hose Fitting | 60 N·m | 43.5 lb ft
Power Steering Gear Inlet Hose Nut | 40 N·m | 29 lb ft
Power Steering Gear Outlet Hose Connector Bolt | 10 N·m | 88.5 lb in
Power Steering Pipe Clamp Bolt | 11 N·m | 96 lb in
Power Steering Pressure Switch (Terminal) | 28 N·m | 20 lb ft
Power Steering Pump Bracket Bolt (1.6L, 2.5L) | 45 N·m | 33 lb ft
Power Steering Pump Bracket Bolt (2.0L) | 25 N·m | 18.5 lb ft
Power Steering Pump Cover Bolts | 23 N·m | 17 lb ft
Power Steering Pump Fitting | 60 N·m | 43.5 lb ft
Power Steering Pump Mount Bolt | 25 N·m | 18.5 lb ft
Steering Shaft Coupling Bolt | 25 N·m | 18 lb ft
Tie Rod Lock Nut | 65 N·m | 47 lb ft