For 1990-2009 cars

### Circuit Description

The DTC P0117 Engine Coolant Temperature (ECT) Sensor Circuit Low Voltage diagnostic monitors the ECT sensor signal. The ECT sensor is a thermistor, a variable resistor whose conductive value changes with the engine coolant temperature, in series with a fixed resistor in the powertrain control module (PCM). The PCM applies 5 volts to the ECT sensor. The PCM monitors the voltage across the ECT sensor and converts the voltage into a temperature reading. When the engine is cold the ECT sensor resistance is high, and when the engine is warm the ECT sensor resistance is low. Therefore, when the engine is cold the PCM will receive a high voltage input, and when the engine is warm the PCM will receive a low voltage input.

Temperature | ECT Resistance | ECT Signal Voltage
--- | --- | ---
Cold | High | High
Warm | Low | Low

### Condition for Running the DTC

The ignition is ON or the engine is running.

### Conditions for Setting the DTC

• | The ECT sensor signal indicates an engine coolant temperature of more than 137°C (279°F).

• | The above condition is met for at least 5 seconds.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL).

• | The PCM records the operating conditions at the time the diagnostic fails. This information will be stored in the Freeze Frame buffer.

• | The PCM enters the Failsafe mode and assumes the engine coolant temperature is 31°C (88°F).

### Conditions for Clearing the MIL/DTC

• | The MIL turns OFF after 3 consecutively passing cycles without a fault present.

• | A history DTC will clear after 40 consecutive warm-up cycles without a fault.

• | Perform the scan tool clear DTC Information function in order to clear the DTC.

### Diagnostic Aids

Check for any of the following conditions:

• | A damaged wiring harness--Inspect the wiring harness for damage. If the harness appears to be OK, observe the ECT display on the scan tool while moving the connectors and the wiring harnesses related to the ECT sensor. A change in the ECT display will indicate the location of the fault.

• | When replacing the ECT sensor, the Temperature vs Resistance Value scale may be used to test the sensor at various temperature levels to evaluate the possibility of a shifted and incorrectly calibrated sensor. A shifted sensor may result in poor driveability complaints. Refer to Temperature Versus Resistance .

• | After the engine is started, the ECT sensor should rise steadily to about 95°C (203°F) and stabilize when the thermostat opens. Verify that the engine is not overheating and has not been subjected to conditions which may create an overheating conditions (i.e., overload, trailer towing, hilly terrain, heavy stop-and-go traffic, etc.).

If DTC P0117 is intermittent, driving the vehicle under the following conditions can verify whether the fault is present. Perform the scan tool clear DTC information function. Road test the vehicle while monitoring the DTC P0117 diagnostic on the scan tool under the Not Ran Since Code Cleared selection in the DTC Information menu. If a DTC P0117 appears in the Not Ran Since Code Cleared list, the P0117 diagnostic has not yet run. When the DTC P0117 does not appear in the Not Ran Since Code Cleared list, the DTC P0117 diagnostic has run. If the MIL is NOT illuminated, and there is no Pending DTC Status in DTC Information, the DTC P0117 diagnostic has passed. The DTCs MUST be cleared in order to view the Current Status of the Not Ran Since Code Cleared list. DO NOT forget that the Not Ran Since Code Cleared list only indicates that the test has run, not whether the test passed or failed. The DTC Information screen must be checked for Current or Pending status, in order to determine the outcome of the diagnostic test involved.

An intermittent malfunction may be caused by a fault in the ETC sensor circuit. Inspect the wiring harness and components for an intermittent condition. Refer to Intermittent Conditions .

If the DTC P0117 cannot be duplicated, the information included in the Freeze Frame data can be useful in determining vehicle operating conditions when the DTC was first set.

### Test Description

The numbers below refer to the step numbers in the diagnostic table.

1. The Diagnostic System Check-Engine Controls prompts the technician to complete some basic checks and store the Freeze Frame data on the scan tool if applicable. This creates an electronic copy of the data taken when the fault occurred. The information is then stored in the scan tool for later reference.

2. This step will determine if a fault is present.

3. Review the Freeze Frame data to determine when the DTC set. Always record this information.

4. This step determines if the fault is caused by a shorted signal circuit or by a malfunctioning ECT sensor.

5. Clearing the DTCs by removing the DOME fuse also clears the PCM long term memory. Using the scan tool to clear DTCs leaves the long term memory active. DTC emitting diagnostics may not run to completion as expected unless the long term memory is cleared. Removal of the DOME fuse also clears the time display of the radio. The DTC P0117 diagnostic can be monitored on the scan tool under the Not Ran Since Code Cleared selection in the DTC Information menu. If a DTC P0117 appears in the Not Ran Since Code Cleared list, the DTC P0117 diagnostic has not yet run. When the DTC P0117 does not appear in the Not Ran Since Code Cleared list, the DTC P0117 diagnostic has run. If the MIL is NOT illuminated, and there is no Pending DTC Status in DTC Information, the DTC P0117 diagnostic has passed. The DTCs MUST be cleared in order to view the Current Status of the Not Ran Since Code Cleared list. DO NOT forget that the Not Ran Since Code Cleared list only indicates that the test has run, not whether the test passed or failed. The DTC Information screen must be checked for Current or Pending status, in order to determine the outcome of the diagnostic test involved.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
Schematic Reference: Engine Controls Schematics
1 | Did you perform the Diagnostic System Check-Engine Controls? | -- | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 |

1. Turn ON the ignition, leaving the engine OFF.
2. Install a scan tool.
3. Observe the engine coolant temperature (ECT) parameter on the scan tool.

Is the ECT more than or equal to the specified value?

205°C (401°F)

Go to Step 4

Go to Step 3

3 |

1. Perform the scan tool Clear DTC Information function.
2. Operate the vehicle within the Freeze Frame conditions as specified.

Is DTC P0117 set?

--

Go to Step 4

Go to Diagnostic Aids

4 |

1. Disconnect the ECT sensor electrical connector.
2. Observe the ECT parameter on the scan tool.

Is the ECT less than or equal to the specified value?

-40°C (-40°F)

Go to Step 6

Go to Step 5

5 |

1. Turn OFF the ignition.
2. Disconnect the PCM electrical connectors.
3. Check the ECT sensor signal circuit for a short to ground.
4. Repair as necessary. Refer to Wiring Repairs in Wiring Systems.

Was a repair necessary?

--

Go to Step 8

Go to Step 7

6 | Replace the ECT sensor. Refer to Engine Coolant Temperature Sensor Replacement . Is the action complete? | -- | Go to Step 8 | --
7 | Replace the PCM. Refer to Powertrain Control Module Replacement . Is the action complete? | -- | Go to Step 8 | --
8 |

1. Turn OFF the ignition.
2. Remove the DOME fuse for 30 seconds.
3. Install the DOME fuse.
4. Reset the radio clock time. Refer to Radio/Audio System Description and Operation in Entertainment.
5. Start the engine.
6. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text or until the DTC P0117 diagnostic test has run.

Does the DTC run and pass?

--

Go to Step 9

Go to Step 2

9 | With a scan tool, observe the stored information, Capture Info. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List | System OK