For 1990-2009 cars

## Folding Top Roof Bow Replacement Front

### Removal Procedure

1. Push in the folding top latch buttons (2).
2. Pull the latch (1) back.
3. Unhook the latch (1) from the folding top #1 bow.
4. Lift the folding top #1 bow.
5. Unsnap the snaps (1) which secure the front folding top material (3) to the folding top #1 bow (4).
6. Unsnap the snap (3) which secures each tension strap (1).
7. Pull the straps (1) out of the plastic loops (2).
8. Remove the 2 screws (2) which secure each side of the folding top #1 bow (1).
9. Remove the folding top #1 bow (1) from the vehicle.

### Installation Procedure

1. Install the folding top #1 bow (1) to the vehicle. Secure the bow with the 2 screws (2) at each side.
2. Pull the tension straps (1) through the plastic loops (2). Secure each strap by snapping the snap (3).
3. Snap the folding top material (3) to the folding top #1 bow (4).
4. Move the folding top #1 bow (4) forward.
5. Hook the folding top #1 bow to the folding top latches (1).
6. Push the latches (1) down until the latches click into place.

## Folding Top Roof Bow Replacement Rear

### Removal Procedure

1. Remove the folding top quarter windows. Refer to Folding Top Quarter Window Replacement .
2. Push down on the release button (1) on each side and tilt the base (2) of the folding top #3 bow (3) forward.
3. Unsnap the rear folding top material from the folding top #3 bow (3).
4. Remove the folding top #3 bow mounting screw trim cover (4) from each side of the vehicle.
5. Remove the two screws which secure each side of the folding top #3 bow (3) to the body.
6. Remove the folding top #3 bow (3) from the vehicle.

### Installation Procedure

1. Install the folding top #3 bow (3) to the vehicle. Secure the bow with the 2 screws at each side.
2. Install the folding top #3 bow mounting screw trim cover (4) to each side of the vehicle.
3. Snap the rear folding top material to the folding top #3 bow (3).
4. Position the folding top #3 bow base (2) rearward and install the folding top #3 bow back to the upright position. Ensure that the release button (1) is fully engaged.
5. Install the folding top quarter windows. Refer to Folding Top Quarter Window Replacement .