For 1990-2009 cars

### Removal Procedure

1. Remove the following components from the instrument panel:

1.1. | The 3 screws (2)

1.2. | The IP steering column opening trim plate (1)

2. Remove the following components from the vehicle:

2.1. | The 4 bolts (1 or 4)

2.2. | The IP drivers knee bolster panel (2 or 3)

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the IP drivers knee bolster panel (2 or 3). Secure the panel with the 4 bolts (1 or 4).

Tighten
Tighten the knee bolster panel bolts to 20 N·m (15 lb ft).

2. Install the IP steering column opening trim plate (1) to the instrument panel. Secure the trim plate with the 3 screws (2).