For 1990-2009 cars

Inspect the following components and the following conditions:

• | The tires for the proper inflation

• | The wheel alignment

• | The wheel bearings for wear or damage

• | The coupling from the column to the steering gear for damage, wear, and improper installation

• | The tie rod ends for free movement

• | The ball joints for free movement

• | The steering shaft bearings for free movement

• | The ball studs for lack of lubrication

• | The tie rod ends for lack of lubrication

• | The ball studs for binding

• | The steering column for binding

• | The flow control valve for sticking and improper operation

• | The steering gear for binding