For 1990-2009 cars

Point | Location | Clearance Gap | Flushness
--- | --- | --- | ---
1 | Windshield Pillar to Windshield | 5.2 mm (0.20 in) | 0-1.5 mm (0.0-.05 in)
2 | Hood to Front Upper Panel | 4.2-7.0 mm (0.16-0.27 in) | 0.0-1.5 mm (0.0-0.05 in)
3 | Hood to Front Fender | 4.5-7.1 mm (0.17-0.28 in) | 0-1.5 mm (0.0-.05 in)
4 | Hood to Air Inlet Grille Panel | 3.7 mm (0.14 in) | N/A
5 | Air Inlet Grille Panel to Front Fender | 4.8 mm (0.18 in) | N/A