For 1990-2009 cars

Inspect the following components and the following conditions:

• | The tires for the proper inflation

• | The coupling from the column to the steering gear for damage, wear, and improper installation

• | The power steering pump for the sufficient pressure output

• | The power steering pump for internal leakage

• | The steering gear for internal leakage

• | The power steering hydraulic system

• | The steering gear for binding and rough movement

• | The steering gear mounting for the proper and secure installation