For 1990-2009 cars

### Removal Procedure

1. Position the front seat assemblies forward in order to gain the necessary clearance to remove the rear floor console screws.
2. Raise the park brake lever in order to gain the necessary clearance to remove the rear floor console.
3. Remove the 2 screws which secure the rear floor console and lift the console.
4. Disconnect the accessory socket electrical connector, if equipped.
5. Remove the rear floor console from the vehicle.

### Installation Procedure

1. Connect the accessory socket electrical connector, if equipped.
2. Install the rear floor console to vehicle. Secure the console with the 2 screws.
3. Lower the park brake lever.
4. Reposition the front seat assemblies backward and in a upright position.