For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable (1).
2. Remove the following items from the floor:

• | The 4 screws (1,6,3,4)

• | The 2 plastic retaining clips (2,5)

• | The console box

3. Remove the shift lock solenoid electrical connector (3) from under the carpet and disconnect.
4. Remove the shift indicator lamp electrical connector.
5. Remove the shift indicator lamp (1).
6. Remove the shift lock solenoid cover (2).
7. Remove the shift lock solenoid (2) from the manual selector.

### Installation Procedure

1. Install the shift lock solenoid (2) to the manual selector.
2. Install the shift lock solenoid cover (2).
3. Connect the shift indicator lamp electrical connector and the shift lock solenoid connector (3) under the carpet.
4. Install the shift indicator lamp (1).
5. Install the console box to the floor.
6. Secure the console box with the 2 plastic retaining clips (2,5) and the 4 screws (1,6,3,4) .
7. Connect the negative battery cable.