For 1990-2009 cars

### Removal Procedure

1. Remove the front floor console. Refer to Front Floor Console Replacement .
2. Remove the upper bolts/screws (2) from the IP.
3. Remove the lower nuts from the floor.
4. Remove the front floor console bracket (1) from the floor.

### Installation Procedure

1. Align the front floor console bracket (1) to the floor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the lower nuts to the front floor console bracket.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

3. Install the upper bolts/screws (2) to the IP.

Tighten
Tighten the bolts/screws to 2.5 N·m (22 lb in).

4. Install the front floor console. Refer to Front Floor Console Replacement .