For 1990-2009 cars

#### Tools Required

J 23653-SIR Lock Plate Compressor

1. Remove the inflatable restraint steering wheel module coil. Refer to Inflatable Restraint Steering Wheel Module Coil Disassemble - Off Vehicle .
2. Remove the wave washer (1).
3. Remove the bearing retainer using J 23653-SIR and dispose of it.
4. Remove J 23653-SIR from the steering column.
5. Remove the shaft lock shield assembly (1).
6. Remove the turn signal cancel cam assembly (2).
7. Remove the upper bearing spring (3).
8. Remove the upper bearing inner race (4).
9. Remove the inner race (5).