For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1-2 Shift Solenoid (1-2 SS) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views | --
2-3 Shift Solenoid (2-3 SS) Valve | Inside the automatic transaxle | Automatic Transmission Electronic Component Views | --
Automatic Transaxle | Lower left side of the engine compartment | -- | --
Automatic Transmission Shift Lock Solenoid | Inside the steering column near the ignition switch | -- | Automatic Transmission Related Connector End Views
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views | Body Control System Connector End Views
Crank Relay | Right side of Engine Compartment on the radiator support, inboard of the underhood accessory wiring junction block | Power and Grounding Component Views | Power and Grounding Connector End Views
Cruise Control Module | Engine compartment, near the left strut tower | Cruise Control Component Views | Cruise Control Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views | Electrical Center Identification Views
Fusible Link C | Bolted to the starter solenoid | -- | --
Powertrain Control Module (PCM) | Engine compartment, secured in the air cleaner assembly | Engine Controls Component Views | Engine Controls Connector End Views
Rear Side Door Actuator Control Module | Right quarter panel, above the wheelhouse | Power Door Systems Component Views | Power Door Systems Connector End Views
Rear Side Door Actuator Motor | Right quarter panel, above the wheelhouse | Power Door Systems Component Views | --
Starter Motor | Lower front of the engine | -- | --
Starter Solenoid | Lower front of the engine, part of the starter motor assembly | -- | --
Stop Lamp Switch | Mounted to the brake pedal support | Cruise Control Component Views | Lighting Systems Connector End Views
Taillamp | Rear of the vehicle, on both sides | Lighting Systems Component Views | Lighting Systems Connector End Views
Tail/Stop Lamps | Rear of the vehicle, inside both taillamps | Lighting Systems Component Views | Lighting Systems Connector End Views
Turn Signal and Headlamp Dimmer Switch and Windshield Wiper and Windshield Washer Switch | Inside the steering column | Lighting Systems Component Views | Lighting Systems Connector End Views
Transaxle Range Switch | Rear left side of the engine compartment, mounted to the top of the transaxle | Engine Controls Component Views | Automatic Transmission Related Connector End Views
Underhood Accessory Wiring Junction Block | Engine compartment, front of the right wheelhouse, above the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
Vehicle Speed Sensor (VSS) | Lower right rear of the engine compartment, mounted to the right side of the transaxle | Automatic Transmission Electronic Component Views | Automatic Transmission Related Connector End Views
C101 (20 cavities) | IP wiring harness to the engine wiring harness, in the lower left side of the engine compartment, near the EBCM | Harness Routing Views | Inline Harness Connector End Views
C111 (14 cavities) | Engine wiring harness to the automatic transaxle wiring harness, lower left side of the engine compartment, front of the automatic transaxle | Automatic Transmission Electronic Component Views | Automatic Transmission Inline Harness Connector End View
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views | Inline Harness Connector End Views
C201 (48 cavities) | IP wiring harness to the steering column wiring harness, mounted to the left side of the steering column near the base | Harness Routing Views | Inline Harness Connector End Views
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views | Inline Harness Connector End Views
G113 | Engine compartment, left of the starter, along with the battery ground | Harness Routing Views | --
G200 | Right side of the IP, gecured on the underside of the cross car beam, above the park brake assembly | Harness Routing Views | --
G401 | Secured to the lower left D-pillar | -- | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views | --
P101 | On the left side of the bulkhead, right of the left strut tower | Harness Routing Views | --
P400 | Behind the right taillamp | Harness Routing Views | --
P401 | Behind the left taillamp | Harness Routing Views | --
S106 | Engine harness, front left side of the engine compartment approximately 10 cm (4 in) from the PCM breakout | -- | --
S108 | Engine harness, front left side of the engine compartment approximately 8 cm (3 in) from the PCM breakout | -- | --
S203 | IP harness, right side of the IP approximately 9 cm (4 in) from the radio breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S406 | Body harness, left rear of the body approximately 17 cm (7 in) from the P401 breakout | -- | --
S435 | Body harness, left rear of the body approximately 26 cm (10 in) from the P401 breakout | -- | --