For 1990-2009 cars

## Rear Wheel Bearing and Hub Replacement Domestic

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
4. Remove and DISCARD the wheel bearing/hub bolts.
5. Remove the wheel bearing/hub.
6. Disconnect the wheel speed sensor electrical connector (2).

### Installation Procedure

1. Connect the wheel speed sensor electrical connector (2).
2. Install the wheel bearing/hub.

Notice: Refer to Fastener Notice in the Preface section.

Caution: These fasteners MUST be replaced with new fasteners anytime they become loose or are removed. Failure to replace these fasteners after they become loose or are removed may cause loss of vehicle control and personal injury.

3. Install the NEW wheel bearing/hub bolts.

Tighten
Tighten the NEW wheel bearing/hub bolts to 80 N·m (59 lb ft).

4. Install the brake drum. Refer to Brake Drum Replacement in Drum Brakes.
5. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
6. Lower the vehicle.

## Rear Wheel Bearing and Hub Replacement Export

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Disconnect the wheel speed sensor electrical connector.
4. Remove the brake caliper bracket with the brake caliper. Refer to Rear Brake Rotor Replacement in Disc Brakes.
5. Remove the brake rotor.
6. Loosen the park brake cable bracket bolts. Do NOT remove the park brake cable bracket bolts. Refer to Park Brake Cable Mounting Bracket Replacement in Park Brake.
7. Remove and DISCARD the wheel bearing/hub bolts.
8. Remove the wheel bearing/hub.
9. Disconnect the wheel speed sensor electrical connector (2).

### Installation Procedure

1. Connect the wheel speed sensor electrical connector (2).
2. Install the wheel bearing/hub.

Caution: These fasteners MUST be replaced with new fasteners anytime they become loose or are removed. Failure to replace these fasteners after they become loose or are removed may cause loss of vehicle control and personal injury.

3. Install the NEW wheel bearing/hub bolts.

Tighten
Tighten the NEW wheel bearing/hub bolts to 85 N·m (63 lb ft).

4. Tighten the park brake cable bracket bolts. Refer to Park Brake Cable Mounting Bracket Replacement in Park Brake.
5. Install the brake rotor.
6. Install the brake caliper bracket with the brake caliper. Refer to Front Brake Rotor Replacement in Disc Brakes.
7. Install the tire and wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
8. Lower the vehicle.