For 1990-2009 cars

## Cargo Net Replacement Upper

### Removal Procedure

1. Open the liftgate.
2. Remove the convenience net from the retainers.
3. Remove the screw from the upper convenience net retainer.
4. Remove the upper convenience net retainer from the body.

### Installation Procedure

1. Install the upper convenience net retainer to the body.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screw to the upper convenience net retainer.

Tighten
Tighten the upper cargo net retainer screws to 2 N·m (18 lb in).

3. Install the convenience net to the retainers.
4. Close the liftgate.

## Cargo Net Replacement Lower

### Removal Procedure

1. Open the liftgate.
2. Remove the convenience net from the retainers.
3. Remove the nut from the floor convenience net retainer stud.
4. Remove the convenience net floor retainer from the floor.

### Installation Procedure

1. Install the convenience net floor retainer to the stud in the floor.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the nut to the floor convenience net retainer stud.

Tighten
Tighten the lower cargo net retainer nut to 10 N·m (89 lb in).

3. Install the convenience net to the retainers.
4. Close the liftgate.