For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror face. Refer to Outside Rearview Mirror Glass Replacement .
2. Remove the outside rearview mirror motor screws.
3. Disconnect the electrical connector.
4. Remove the outside rearview mirror motor from the mirror housing.

### Installation Procedure

1. position the outside rearview mirror motor to the mirror housing.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the outside rearview mirror motor screws.

Tighten
Tighten the screws to 10 N·m (89 lb in).

3. Connect the electrical connector.
4. Install the outside rearview mirror face. Refer to Outside Rearview Mirror Glass Replacement .