For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Ambient Air Temperature Sensor | In front of the radiator, right side | HVAC Component Views in HVAC Systems-Manual | HVAC Connector End Views in HVAC Systems-Manual
Body Control Module (BCM) | Below the right side of the IP, right of the IP compartment | Body Control System Component Views in Body Control Systems | Body Control System Connector End Views in Body Control Systems
Data Link Connector (DLC) | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Driver Information Display | In the roof console | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Fuse Block | Right side of the IP, in the right front door opening | Power and Grounding Component Views in Wiring Systems | Electrical Center Identification Views in Wiring Systems
Instrument Cluster | Left side of the IP | Instrument Panel, Gages, and Console Component Views | Instrument Panel, Gages, and Console Connector End Views
Splice Pack SP205 | Below the steering column, bottom of the knee bolster | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
C120 (3 cavities) | IP wiring harness to the forward lamp wiring harness, between the battery and the windshield fluid reservoir | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (56 cavities) | IP wiring harness to the right side of the body wiring harness, behind the right side of the IP compartment, below P100 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (56 cavities) | IP wiring harness to the left side of the body wiring harness, left side of the steering column, below P101 | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C305 (12 cavities) | Body wiring harness to the electronic brake control wiring harness and fuel sender wiring harness, mounted as a pass through, beneath the vehicle behind the driver seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C308 (23 cavities) | Body wiring harness to the roof wiring harness, inside the right B-pillar, behind the lower trim | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G200 | Right side of the IP, secured on the underside of the cross car beam, left of the heater-A/C vent | Harness Routing Views in Wiring Systems | --
P100 | On the right side of the bulkhead, left of the right strut tower | Harness Routing Views in Wiring Systems | --
S202 | IP harness, leftt side of the IP approximately 15 cm (6 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S209 | IP harness, center of the IP approximately 8 cm (3 in) from the security indicator lamp breakout | -- | --
S210 | IP harness, center of the IP approximately 4 cm (2 in) from the security indicator lamp breakout | -- | --
S211 | IP harness, left side of the IP approximately 15 cm (6 in) from the radio and the rear window wiper/washer and multi-function switch breakout | -- | --
S230 | IP harness, right side of the IP approximately 4 cm (2 in) from the rear window wiper/washer and multi-function switch breakout | -- | --
S264 | IP harness, right side of the IP approximately 16 cm (6 in) from the relay center breakout | -- | --
S326 | Body harness, top/forward area of the left rear wheel well approximately 13 cm (5 in) behind the second oval clamp | -- | --