For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooler Pipe Retainer Bolt/Screw | 10 N·m | 89 lb in
Power Steering Cooler Hose/Pipe Fittings | 27 N·m | 20 lb ft
Power Steering Gear Nuts (at Frame) * | 80 N·m | 59 lb ft
Power Steering Pump Bolts | 34 N·m | 25 lb ft
Steering Intermediate Shaft Lower (Pinch) Bolt | 45 N·m | 33 lb ft
Tie Rod Ball Stud Nut * | 30 N·m + 120 degrees (2 flats) ¹ | 22 lb ft + 120 degrees (2 flats) ¹
* This is a prevailing torque type fastener. This fastener may be reused ONLY if:

• | The fastener and its counterpart are clean and free from rust

• | The fastener develops a specified amount of torque (drag) against its counterpart prior to the fastener seating.

| Refer to the appropriate service procedure for the prevailing torque value.

If the fastener does not meet these criteria, REPLACE the fastener.

¹ Ensure that 2.5--4.5 tie rod end threads are visible beyond the tie rod ball stud nut nylon.