For 1990-2009 cars

### Removal Procedure

1. Remove the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.
2. Disconnect the electrical connector from the switch (1).
3. Pull out the switch (1) in order to remove the switch (1) from the retainer in the brake pedal bracket.

### Installation Procedure

1. Push in the switch (1) in order to install the switch (1) to the retainer in the brake pedal bracket.
2. Connect the electrical connector to the switch (1).
3. Adjust the cruise control release switch and the stoplamp switch. Refer to Cruise Release Switch Adjustment .
4. Install the left instrument panel insulator. Refer to Instrument Panel Insulator Panel Replacement - Left Side in Instrument Panel, Gauges and Console.