For 1990-2009 cars

### Removal Procedure

1. Disconnect the battery ground (negative) cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls - 3.4L.
3. Remove the right engine mount strut. Refer to Engine Mount Strut Replacement in Engine Mechanical.
4. Install the engine support fixture. Refer to Engine Support Fixture in Engine Mechanical.
5. Disconnect the transaxle wiring harness connectors.
6. Remove the automatic transaxle range selector cable from the cable lever. Refer to Range Selector Lever Cable Replacement .
7. Remove the automatic transaxle range selector cable bracket with cable from the transaxle. Refer to Range Selector Lever Cable Bracket Replacement .
8. Remove the PNP switch. Refer to Park/Neutral Position Switch Replacement .
9. Remove the fluid filler tube. Refer to Transmission Fluid Filler Tube Replacement .
10. Remove the upper transaxle bolts (3, 4 and 5) and stud (2).
11. Remove the wiring harness grounds.
12. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
13. Remove the front tires and wheels. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
14. Remove the engine splash shields. Refer to Engine Splash Shield Replacement in Body Front End.
15. Remove the torque converter cover. Refer to Torque Converter Cover Replacement .
16. Remove the starter motor. Refer to Starter Motor Replacement in Engine Electrical.
17. Remove the flywheel to torque converter bolts. Refer to Flywheel to Torque Converter Bolt Replacement .
18. Disconnect the transaxle oil cooler hoses from the transaxle. Refer to Automatic Transmission Oil Cooler Hose Replacement .
19. Disconnect the drive axles from the transaxle. Refer to Wheel Drive Shaft Replacement in Front Wheel Drive Shafts.
20. Use straps or wire in order to support the drive axles.
21. Disconnect the vehicle speed sensor connector. Refer to Input Speed Sensor Replacement .
22. Remove the transaxle brace. Refer to Transmission Brace Replacement .
23. Remove the frame. Refer to Frame Replacement in Frame and Underbody.
24. Use the transmission jack in order to support the transaxle.
25. Remove the utility strap from ONLY the transaxle.
26. Remove the lower transaxle bolt (6) and stud (1).
27. Separate the transmission from the engine.
28. Use the transmission jack in order to lower the transmission.
29. Flush the transaxle oil cooling system. Refer to Transmission Fluid Cooler Flushing .

### Installation Procedure

1. Use the transmission jack in order to raise the transmission.
2. Install the transmission to the engine.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the transaxle lower bolt (6) and stud (1).

Tighten
Tighten the transaxle lower bolt and stud to 75 N·m (55 lb ft).

4. Install the utility strap to the transaxle.
5. Tighten the utility strap in order to prevent the rotation (movement) of the powertrain.
6. Install the transaxle brace. Refer to Transmission Brace Replacement .
7. Install the drive axles to the transaxle. Refer to Wheel Drive Shaft Replacement in Front Wheel Drive Shafts.
8. Remove the transmission jack.
9. Install the frame. Refer to Frame Replacement in Frame and Underbody.
10. Remove the support straps from the vehicle.
11. Install the transaxle oil cooler hoses to the transaxle. Refer to Automatic Transmission Oil Cooler Hose Replacement .
12. Install the flywheel to torque converter bolts. Refer to Flywheel to Torque Converter Bolt Replacement .
13. Install the starter motor. Refer to Starter Motor Replacement in Engine Electrical.
14. Install the torque converter cover. Refer to Torque Converter Cover Replacement .
15. Install the engine splash shields. Refer to Engine Splash Shield Replacement in Body Front End.
16. Install the front tires and wheels. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
17. Lower the vehicle.
18. Install the wiring harness grounds.
19. Install the upper transaxle bolts (3, 4, 5) and stud (2).

Tighten
Tighten the bolts and stud to 75 N·m (55 lb ft).

20. Install the fluid filler tube. Refer to Transmission Fluid Filler Tube Replacement .
21. Install the PNP switch. Refer to Park/Neutral Position Switch Replacement .
22. Install the automatic transaxle range selector cable bracket with cable to the transaxle. Refer to Range Selector Lever Cable Bracket Replacement .
23. Install the automatic transaxle range selector cable to the cable lever. Refer to Automatic Transmission Range Selector Lever Replacement .
24. Install the transaxle wiring harness connectors.
25. Remove the engine support fixture. Refer to Engine Support Fixture in Engine Mechanical.
26. Install the right engine mount strut. Refer to Engine Mount Strut Replacement in Engine Mechanical.
27. Install the throttle body air inlet duct. Refer to Air Cleaner Assembly Replacement in Engine Controls - 3.4L.

Important: It is recommended that transmission adaptive pressure (TAP) information be reset.

Resetting the TAP values using a scan tool will erase all learned values in all cells. As a result, The ECM, PCM or TCM will need to relearn TAP values. Transmission performance may be affected as new TAP values are learned.
28. Reset the TAP values. Refer to Adapt Function .