For 1990-2009 cars

### Removal Procedure

1. Disconnect the MAF sensor electrical connector.
2. Loosen the air intake duct/MAF sensor hose clamps.
3. Remove the air intake duct/MAF sensor assembly (1).
4. Unsnap the 2 housing cover retaining clamps.
5. Remove the air cleaner cover (2) and carefully remove the air filter element (3).
6. Inspect the housing cover, seal assembly, and air ducting for damage. If a problem is found, replace as necessary.

### Installation Procedure

1. Carefully install the air filter element (3) into the air cleaner assembly.
2. Install the housing cover (2) and snap the retaining clamps in place.
3. Install the air intake duct/MAF sensor assembly (1).
4. Tighten the air intake duct/MAF sensor hose clamps.
5. Connect the MAF sensor electrical connector.