For 1990-2009 cars

### Removal Procedure

1. Open and support the hood.
2. Remove the wing nut from the headlamp bracket.
3. Remove the front park/turn signal/sidemarker lamp from the fender.
4. Press the tab while turning counterclockwise to remove the bulb socket from the front park/turn signal/sidemarker lamp.
5. Pull the bulb from the socket.

### Installation Procedure

1. Press the bulb into the socket.
2. Install the socket to the front park/turn signal/sidemarker lamp.
3. Position the front park/turn signal/sidemarker lamp to the fender:

3.1. | Locate the tabs into the fender.

3.2. | Install the tab into the headlamp bracket.

4. Install the wing nut to headlamp bracket and hand tighten.
5. Close the hood.