For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Door Trim Panel Replacement .
2. Lower the front door window.
3. Remove the front door inner belt window sealing strip by lifting off the pinch-weld flange.

### Installation Procedure

Important: Install the front door weather-strip before installing the front door inner belt window sealing strip.

1. Install the front door inner belt sealing strip to the pinch-weld flange.
2. Install the front door trim panel. Refer to Door Trim Panel Replacement .
3. Raise the front door window.