For 1990-2009 cars

### Removal Procedure

1. Remove the rear fan/temperature control from the rear overhead console using a small flat-bladed tool to pry and release the mounting tabs of the control.
2. Disconnect the electrical connectors from the control.

### Installation Procedure

1. Connect the electrical connectors to the rear fan/temperature control.
2. Install the control by pushing the control into the console until the retaining tabs snap into place.