For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the lighting diagnostic system check? | -- | Go to Step 2 | Go to Diagnostic System Check - Lighting Systems
2 | Is the left turn signal and high beam indicators on also? | -- | Go to Step 3 | Go to Step 4
3 | Repair the open in the ground circuit of the IPC. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Step 6 | --
4 | Is the right turn lamp illuminated? | -- | Go to Diagnostic System Check - Lighting Systems | Go to Step 5
5 | Replace the IPC. Refer to Instrument Cluster Replacement in Instrument Panel, Gauges, and Console. Important: Perform the set up procedure for the IP. Did you complete the replacement and the set up procedure? | -- | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2