For 1990-2009 cars

### Removal Procedure

1. Rotate the drive belt tensioner in order to release the tension on the drive belt.
2. Remove the drive belt.

### Installation Procedure

1. Install the drive belt to all of the pulleys except the generator pulley.
2. Rotate the drive belt tensioner in order to install the drive belt over the generator pulley.

Important: Ensure that the drive belt is aligned into the proper grooves of the accessory drive belt pulleys.

3. Ensure that the drive belt is properly routed.