For 1990-2009 cars

1. Remove the automatic transmission shift lock control assembly. Refer to Automatic Transmission Shift Lock Control Disassemble - Off Vehicle .
2. Remove the park lock cable assembly (1) from the electronic lock module assembly.
3. Remove the hexagon flanged head bolt.
4. Remove the ball and actuator assembly (2).
5. Remove the shift lever clevis (1).
6. Remove the 2 oval head 6-lobed socket tapping screws from the shift gate.
7. Remove the hexagon flange head bolt.
8. Remove the cable shift cam assembly (1).
9. Remove the cam bushing (2) from the cable shift cam assembly (1).
10. Remove the 3 flat head 6-lobed socket tapping screws.
11. Remove the gearshift lever assembly support bracket.