For 1990-2009 cars

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the coolant. Refer to Cooling System Draining and Filling .
2. Disconnect the outlet hose from the water pump housing using the J 38185 .
3. Disconnect the outlet hose from the radiator using the J 38185 .
4. Remove the outlet hose.

### Installation Procedure

1. Install the outlet hose in position and align the marks on the hose.
2. Connect the outlet hose to the radiator using the J 38185 .
3. Connect the outlet hose to the water pump housing using the J 38185 .

Important: To properly fill the system you must use of the air bleed vents.

4. Refill the coolant. Refer to Cooling System Draining and Filling .