For 1990-2009 cars

### Removal Procedure

1. Remove the liftgate trim panel. Refer to Liftgate Trim Panel Replacement in Body Rear End.
2. Remove the rear radio speaker (1):

2.1. | Push on the top tab.

2.2. | Pull the speaker (1) from the liftgate (2).

3. Disconnect the electrical connector from the rear radio speaker.

### Installation Procedure

1. Connect the electrical connector to the rear radio speaker.
2. Install the rear radio speaker (1):

2.1. | Insert the tabs into the lower slots.

2.2. | Push the upper tab into the slot on the liftgate (2).

3. Install the liftgate trim panel. Refer to Liftgate Trim Panel Replacement in Body Rear End.