For 1990-2009 cars

### Removal Procedure

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
2. Remove the fuse block IP end caps.
3. Release the front retainer on the fuse block.
4. Push the fuse block into the instrument panel.
5. Remove the fuse block from the instrument panel.
6. Remove the electrical connectors from the fuse block. Refer to Connector Repairs in Wiring Systems.

### Installation Procedure

1. Install the electrical connectors into the fuse block. Refer to Connector Repairs in Wiring Systems.
2. Align the rear side of the fuse block with the instrument panel.
3. Push the fuse block into the opening until secure.
4. Install the IP end caps.
5. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.