For 1990-2009 cars

#### Tools Required

J 36850 Assembly Lubricant (or equivalent)

1. Use J 36850 or equivalent in order to secure the second clutch housing thrust washer (611) to the driven sprocket support assembly (609).
2. Finger start two 13 mm case cover bolts (434) into the driven sprocket support assembly (609).

Important: If the driven sprocket support assembly (609) is not flush with or slightly below the case, then one of the clutches is not fully seated.

3. Using the bolts (434), lift the driven sprocket support assembly (609) into the case and align as shown. The top of the driven sprocket support assembly (609) should be flush with the case.