For 1990-2009 cars

Refer to Engine Controls Schematics .

#### I/P, Generator and Driver Information Display

Power, Ground and Door Locks
Power/Ground Distribution, Instrument Cluster and DID
Turn Signal Switch, PCM, IPC and Engine Oil Pressure Switch
DRL, Canister, PWR DROP, TURN, SIR, IP-IGN, CRUISE, and ECM Fuse
DRL, Canister, PWR DROP, TURN, SIR, IP-IGN, CRUISE, and ECM Fuse
Handling ESD Sensitive Parts Notice
G200 (4 of 4)
G200 (3 of 4)
Instrument Cluster Indicators, MSVA and Stop Lamp Switch
Handling ESD Sensitive Parts Notice
Engine Controls Components
Powertrain Control Module Description
IAC, I/P, Engine Oil Level Indicator Switch and PNP
MAF, EGR, EVAP Purge and EVAP Canister Valve
OBD II Symbol Description Notice
.

### Circuit Description

The PCM Output (L) terminal to the alternator determines when the alternator will be turned off. It is on under all normal vehicle operating conditions except during low RPM conditions. The alternator is turned off during low RPM conditions to remove excess load from the engine.

The alternator telltale lamp will illuminate any time the ignition is on and engine is not running. The telltale will go out after the engine is running and the alternator is putting out the desired amperage.

### Conditions for Running the DTC

• | The engine is running.

• | The voltage telltale is ON.

### Conditions for Setting the DTC

• | (L) terminal voltage is low while the PCM is commanding the generator on.

• | The above condition is present for more than 10 seconds.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL) on the second consecutive ignition cycle that the diagnostic runs and fails.

• | The PCM records the operating conditions at the time the diagnostic fails. The first time the diagnostic fails, the PCM stores this information in the Failure Records. If the diagnostic reports a failure on the second consecutive ignition cycle, the PCM records the operating conditions at the time of the failure.

• | The PCM writes the conditions to the Freeze Frame and updates the Failure Records.

### Conditions for Clearing the MIL/DTC

• | The PCM will turn OFF the malfunction indicator lamp (MIL) during the third consecutive trip in which the diagnostic has run and passed.

• | The history DTC will clear after 40 consecutive warm-up cycles have occurred without a malfunction.

• | The DTC can be cleared by using a scan tool.

### Diagnostic Aids

Check for the following conditions:

Many situations may lead to an intermittent condition. Perform each inspection or test as directed.

Important: : Remove any debris from the connector surfaces before servicing a component. Inspect the connector gaskets when diagnosing or replacing a component. Ensure that the gaskets are installed correctly. The gaskets prevent contaminate intrusion.

• | Loose terminal connection

- | Use a corresponding mating terminal to test for proper tension. Refer to Testing for Intermittent Conditions and Poor Connections , and to Connector Repairs in Wiring Systems for diagnosis and repair.

- | Inspect the harness connectors for backed out terminals, improper mating, broken locks, improperly formed or damaged terminals, and faulty terminal to wire connection. Refer to Testing for Intermittent Conditions and Poor Connections , and to Connector Repairs in Wiring Systems for diagnosis and repair.

• | Damaged harness--Inspect the wiring harness for damage. If the harness inspection does not reveal a problem, observe the display on the scan tool while moving connectors and wiring harnesses related to the sensor. A change in the scan tool display may indicate the location of the fault. Refer to Wiring Repairs in Wiring Systems for diagnosis and repair.

• | Inspect the powertrain control module (PCM) and the engine grounds for clean and secure connections. Refer to Wiring Repairs in Wiring Systems for diagnosis and repair.

If the condition is determined to be intermittent, reviewing the Snapshot or Freeze Frame/Failure Records may be useful in determining when the DTC or condition was identified.

### Test Description

The numbers below refers to the step number on the diagnostic table:

1. This vehicle is equipped with a PCM which utilizes and electrically erasable programmable read only memory (EEPROM). When the PCM is being replaces, the new PCM must be programmed.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On Board Diagnostic (OBD) System Check? | -- | Go To Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Start the engine and let idle.
2. Using scan tool, monitor Commanded Generator.

Does the scan tool indicate that the Commanded Generator is on?

--

Go To Step 4

Go To Step 3

3 |

1. Turn OFF the ignition.
2. Disconnect the Generator harness connector.
3. Connect a DMM between the (L) terminal at the harness connector and a known good ground.
4. Start the engine.

Command the Generator on with the scan tool while monitoring the DMM.

Does the voltage change from the first indicated value to the second indicated value?

0.0-V

5.0-V

Go to Diagnostic System Check - Engine Electrical in Engine Electrical

Go To Step 4

4 | Test the (L) circuit for an open or short to ground and repair if necessary. Refer to Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go To Step 8 | Go To Step 5
5 | Test the (L) circuit for a short to voltage and repair if necessary. Refer to Wiring Repairs in Wiring Systems. Did you find and correct the condition? | -- | Go To Step 8 | Go To Step 6
6 | Inspect for a poor connection at the PCM and repair if necessary. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems. Did you find and correct the condition? | -- | Go To Step 8 | Go To Step 7
7 | Important: : The replacement PCM must be programmed. Replace the PCM. Refer to Powertrain Control Module Replacement/Programming . Did you complete the repair? | -- | Go To Step 8 | --
8 |

1. Review and record scan tool Fail Records data.
2. Clear DTCs.
3. Operate the vehicle within Fail Records conditions as noted.
4. Using a scan tool, monitor Specific DTC info for DTC P0620.

Does the scan tool indicate DTC P0620 failed this ignition?

--

Go To Step 2

System OK