For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coolant Heater Bolt/Screw | 2 N·m | 18 lb in
Cooling Fan Nut | 6 N·m | 53 lb in
Cooling Fan Motor Screws | 6 N·m | 53 lb in
Cooling Fan Shroud Bolts | 6 N·m | 53 lb in
Radiator Bracket Bolts | 24 N·m | 18 lb ft
Radiator Lower Air Deflector Bolts | 20 N·m | 15 lb ft
Thermostat Bypass Pipe Bolt | 11 N·m | 98 lb in
Thermostat Bypass Pipe Nut | 25 N·m | 18 lb ft
Thermostat Housing Bolts | 25 N·m | 18 lb ft
Water Pump Bolts | 10 N·m | 89 lb in
Water Pump Pulley Bolts | 25 N·m | 18 lb ft