For 1990-2009 cars

Causes | Correction
--- | ---
Sticky caliper or caliper pistons | Repair/replace the caliper.
Contaminated/improper brake fluid | Flush the brake system and repair the affected brake components.
Uneven brake lining material | Replace the brake linings.
Front and/or rear brake assembly attachment loose | Locate and tighten the loose brake components.
Restricted brake fluid passage | Locate and fix the source of the brake fluid restriction.
Improperly adjusted stoplamp switch | Adjust the stoplamp switch to specification.
Brake pedal linkage interference/binding | Repair/replace the brake pedal linkage.
Improperly adjusted parking brake | Adjust the parking brake.
Loose front suspension parts | Locate and tighten/repair/replace the loose front suspension components.
Operator riding the brake pedal | Advise the operator of proper brake usage.
Missing or weak pedal-return spring | Replace the pedal-return spring
Improperly adjusted booster push rod | Adjust the booster push rod.