For 1990-2009 cars

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Partially drain the coolant. Refer to Cooling System Draining and Filling .
2. Disconnect the inlet hose from the thermostat housing using the J 38185 .
3. Disconnect the inlet hose from the radiator using the J 38185 .
4. Remove the inlet hose.

### Installation Procedure

1. Install the inlet hose in position and align the marks on the hose.
2. Connect the inlet hose to the radiator using the J 38185 .
3. Connect the inlet hose to the thermostat housing using the J 38185 .

Important: To properly fill the system you must use of the air bleed vents.

4. Refill the coolant. Refer to Cooling System Draining and Filling .