For 1990-2009 cars

### Removal Procedure

1. Remove the body pillar upper trim panel. Refer to Center Pillar Upper Trim Panel Replacement .
2. Remove the assist handle retaining bolts.
3. Remove the assist handle from the vehicle.

### Installation Procedure

1. Install the assist handle to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the assist handle retaining bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the body pillar upper trim panel. Refer to Center Pillar Upper Trim Panel Replacement .