For 1990-2009 cars

#### Tools Required

• | J 29130 Axle Seal Installer

• | J 8092 Driver Handle

Notice: Install the seal onto the tool before installing into the case to prevent damage to the seal.

Important: Inspect the axle oil seal assembly (4). Be sure that the seal was not damaged during assembly. Check that the garter spring was not dislodged.

Use J 29130 and J 8092 in order to install the axle oil seal assembly (4) on the case extension assembly.